**Questions:**

1. What is the square footage for the entire indoor playing area taking into consideration removing the electric panels in the north east corner so we could have playing surfaces up against the east wall?
2. What is the height of ceiling in the non-playing area- the office/rental space areas?
3. What is the total square footage of the commercial office space on the west side of the building?

**Layout Changes:**

1. One large soccer field without knowing the square footage we are estimating 180 X 80

(We will be dividing this area into 3 small fields ideally)

1. 4 volleyball courts 3 running N/S 1 running W/E (VB courts are 30 X 60 – 3 feet of clearance around court area needed)
2. 2 basketball courts running N/S Basketball courts are 94 X 50 (3 feet of clearance around court area needed)
3. Remove drawings of the track and batting cages put in a soccer field
4. Main Entrance is located in center of building

6-16 maybe difficult to understand. We are trying to lay out the south side of the building. We may just have to review over the phone or on Monday.

1. Main entrance will lead to our front desk area
2. Next to the front desk will be the concession area (serving area/prep areas/sinks)
3. Behind the concession area on the South facing walls are staff offices
4. Staff offices consist of 2 offices 10 X 10 or 12 X 12 and an area for 4 cubes/stations
5. Seating Area for Concessions/Spectators to follow and can extend close to playing
6. Next in line one large meeting room that can be split into 2 – entire space approx. 40 X 12
7. Followed by Restrooms – 2 showers per restroom. Restroom set up Sinks, Toilets, Showers, Lockers (similar to the drawings only smaller)
8. Mechanics Room- Washer Dryer, Cleaning Supplies, etc. to line up next to restrooms
9. Equipment Storage area in corner near courts
10. Equipment Storage area opposite corner near field
11. How do we have access to the electrical panel in the southwest corner if those spaces are being leased out?

**Outdoor Area**

1. 2 sand volleyball courts out of northwest corner of building – courts will run North and South
2. Turf Field Running East to West – bummer but we don’t see another way to do it.
3. Concession structure attached to building near playing areas (approx. 800 square feet)
4. 2 Unisex outdoor bathrooms attached to building or concession area (or whatever quantity is needed for code)
5. Deck/Patio Area for seating and viewing
6. Entire outdoor area is fenced in